**PCIe connector pin count: -**

|  |  |
| --- | --- |
| Lanes | Pins |
| x1 | 36 |
| x4 | 64 |
| x8 | 98 |
| x16 | 164 |